; Installation inf for the Intel 82930 USB Bulk IO Test Board
;
; (c) Copyright 1999 Microsoft
;

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%MSFT%
DriverVer=02/08/2007

[SourceDisksNames]
1="SkyUsb Installation Disk",,,

[SourceDisksFiles]
SKYUSB.SYS = 1
;SKYUSB.INF = 1

[Manufacturer]
%MfgName%=Microsoft

[Microsoft]
%USB\VID_1516&PID_8628.DeviceDesc%=SKYUSB.Dev, USB\VID_1516&PID_8628
;NEW_VID_PID_START

;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
SKYUSB.Files.Ext = 10,System32\Drivers
SKYUSB.Files.Inf = 10,INF

[SKYUSB.Dev]
CopyFiles=SKYUSB.Files.Ext, SKYUSB.Files.Inf
AddReg=SKYUSB.AddReg

[SKYUSB.Dev.NT]
CopyFiles=SKYUSB.Files.Ext, SKYUSB.Files.Inf
AddReg=SKYUSB.AddReg

[SKYUSB.Dev.NT.Services]
Addservice = SKYUSB, 0x00000002, SKYUSB.AddService

[SKYUSB.AddService]
DisplayName    = %SKYUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\SKYUSB.SYS
LoadOrderGroup = Base

[SKYUSB.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SKYUSB.SYS
HKLM,"System\Currentcontrolset\Services\SKYUSB\Parameters","MaximumTransferSize",0x10001,4096
HKLM,"System\Currentcontrolset\Services\SKYUSB\Parameters","DebugLevel",0x10001,0
HKLM,"System\Currentcontrolset\services\SKYUSB\Parameters","BulkUsbEnable",0x10001,0
HKLM,"System\Currentcontrolset\services\SKYUSB\Parameters","CBWTimeOut",0x10001,1000
HKLM,"System\Currentcontrolset\services\SKYUSB\Parameters","CSWTimeOut",0x10001,2000

[SKYUSB.Files.Ext]
SKYUSB.SYS

[SKYUSB.Files.Inf]
;SKYUSB.INF


;---------------------------------------------------------------;

[Strings]
MSFT="Microsoft"
MfgName="Skymedi"
USB\VID_1516&PID_8628.DeviceDesc="SKYMEDI Corp. Generic USB Driver"
SKYUSB.SvcDesc="SKYMEDI Corp. Generic USB Driver"

